		       MOBOTIX M10 UPDATE NOTES
		       ========================


* General Information

  Date:           2006-12-22

  Release:        M10-V2.2.3.24

  For Hardware:   MOBOTIX M10 Network Cameras
                  128 MB RAM

  Manufacturer:   MOBOTIX AG
                  Luxemburger Str. 6
                  67657 Kaiserslautern
                  GERMANY
                  http://www.mobotix.com/



* General Notes

This is an improved customer version for M10 cameras with software M10-V2.2.0.5
or higher.

No warranty for any function.

No warranty for compatibility to former or future versions.

USE ONLY AT YOUR OWN RISK!


The software can be used on all M10/D10 cameras with at least 128 MB RAM
with software version M10-V2.2.0.5 or higher. If you own an M10/D10 with a
software version M10-V2.1.x.x, please contact MOBOTIX support at
support@mobotix.com.

This update will NOT work on M1 or M22 cameras.

News about this software release can be found under this address:

   http://www.mobotix.com/



* Updating the Camera Software

 1. Download the file M10_system_de_2_2324.mpl or the file M10_system_de_2_2324.zip
    to your computer. If you downloaded the zip file, unzip it.

 2. Make sure that the file has been transferred completely. The table at the
    end contains the file size and checksums for the download files.

 3. Make sure that the camera fulfills the requirements listed above. Check
    the information under "Admin Menu > Hardware and Release Information" on the
    camera.

 4. Make sure that you are connected directly to the camera, without any proxy
    server in-between. Disable any proxy servers. Microsoft Internet Explorer:
    "Tools > Internet Options > Connections (tab) > Settings (in LAN Settings) >
    Proxy Server".

 5. Restart the camera.

 6. Log onto the camera as administrator, open "Admin Menu > Upload system
    software from local computer" and read the Important Notes. Select the file
    M10_system_de_2_2324.mpl and start the upload.

    CAUTION:
       - Never disrupt the procedure while the camera is uploading or
         rewriting its flash memory. This may leave the camera operating
         system in an undefined state and prevent the camera from booting.

       - The upload procedure may take several minutes, and up to 30 minutes
         when using an ISDN connection.

       - The camera LEDs will show a rotating pattern while uploading and
         three LEDs will blink when the flash memory is being written.

       - During the procedure, the browser windows may not be updated
         properly.

 7. Upon completion of the upload, the camera will display a message. Read
    this message carefully.

 8. If the upload has finished successfully, restart the camera. If the upload
    was not successful, do not reboot the camera. Restart the upload process and
    wait until the upload has finished successfully.

 9. The settings of the camera will remain intact during and after the update.
    It is recommended, however, to reset certain parts of the configuration to
    the factory defaults, while keeping the other parts of the current
    configuration. If conflicts are detected while opening camera pages, warning
    messages will inform you about these conflicts.

    When resetting the configuration to factory defaults, the network, audio,
    and security settings should not be reset to factory defaults as this may
    render the camera unreachable.



* Files--Overview

    Bytes md5sum                            Name
--------------------------------------------------------------------------
  7986020 9a021c471f025fedb3fba901f3e70da8  M10_system_de_2_2324.mpl
  7803921 6f46bba8c738e6c7bc706005d638354c  M10_system_fr_2_2324.mpl
  8166074 90ef4a5aa3c94156651ff2b3781e64b0  M10_system_it_2_2324.mpl
  7469034 9dd485a7235e4a29a904fc6ffd4d4197  M10_system_jp_2_2324.mpl
  7989583 602a6e0eb786f03a7acf05e21352a08d  M10_system_es_2_2324.mpl
