			Upload to M1-V1.6.5.2
			=====================
	Gerald Eberhard Time-stamp: <2001-05-25 22:00:31 root>


* Preface 

M1-V1.6.5 is the new system software for MOBOTIX M1 released end of
May 2001.


* Installation

** Conditions

- Desable any Proxy-Server 

- Ensure that the camera will not lost power supply while updating.

- The current configuration will be kept over the upate.



** Steps of Installation using M1-V1.6.4.x

1    Reboot the camera

2    If you want to update the camera via ISDN

2.1  Upload M1M_serviceupdate_003.mpl into the camera

2.2  Reboot the camera

2.3  Upload M1M_serviceupdate_005.mpl into the camera

2.4  Reboot the camera


3    Upload M1M_system_1_652.mpl into the camera


4    Reboot the camera

5    The camera will restart with the new software.  In the page
     header the version tag M1-V1.6.5 is shown. More details are shown
     in http://<camera>/admin/version.
     Note: Some browsers keep the pages in their buffer for a longer
     time. Use Shift-Reload to refresh the pages.


** Steps of Installation using M1-V1.5.x and lower

- Upload M1-V1.6.5.1-full.upl. Note that all configuration settings
  will be lost.


Kaiserslautern, 2001-05-25 GEb