                  MOBOTIX FIRMWARE-UPDATE NOTES
                  =============================


* General Information

  Date:           2013-06-11

  Release:        MX-V3.5.5.10

  For Hardware:   MOBOTIX Network Cameras
                  M12-Models (D12, V12, ...)
                  M22-Models (D22, Q22)

  Manufacturer:   MOBOTIX AG
                  Kaiserstrasse
                  67722 Langmeil
                  GERMANY
                  http://www.mobotix.com/


* General Notes

This is an improved customer version for MOBOTIX cameras with software
MX-V3.4.x or higher.

No warranty for any function.

No warranty for compatibility to former or future versions.

USE ONLY AT YOUR OWN RISK!


The software can be used on all M12, D12, V12, M22, D22 und Q22 cameras
and software version MX-V3.4.x or higher.

This update will NOT work on older cameras.

News about this software release can be found under this address:

   http://www.mobotix.com/



* Updating the Camera Software

 1. Download the file MX_system_xx_3_5510.mpl to your computer.

 2. Make sure that the file has been transferred completely. The table at the
    end contains the file size and MD5 checksum for the download file.

 3. Make sure that the camera fulfills the requirements listed above. Check
    the information under "Admin Menu > Hardware and Release Information" on the
    camera.

 4. Make sure that you are connected directly to the camera, without any proxy
    server in-between. Disable any proxy servers. Microsoft Internet Explorer:
    "Tools > Internet Options > Connections (tab) > Settings (in LAN Settings) >
    Proxy Server".

 5. Restart the camera.

 6. Log onto the camera as administrator, open "Admin Menu > Upload system
    Software" and read the Important Notes. Select the file
    MX_system_xx_3_5510.mpl and start the upload.

    CAUTION:
       - Never disrupt the procedure while the camera is uploading or
         rewriting its flash memory. If this has happened anyhow, the camera
         will automatically boot the backup system (the title bar in the browser
         interface is red). The backup system only allows updating the system
         software.

       - The upload procedure may take several minutes, and up to 30 minutes
         when using an ISDN connection.

       - The camera LEDs will show a specific pattern while uploading.
         Please read the manual for the meaning.

       - During the procedure, the browser windows may not be updated
         properly.

 7. Upon completion of the upload, the camera will display a message. Read
    this message carefully.

 8. If the upload has finished successfully, restart the camera. If the upload
    was not successful, do not reboot the camera. Restart the upload process and
    wait until the upload has finished successfully.

    If the camera detects a faulty operating system, it will boot its backup
    operating system (the title bar in the browser interface is red); in this
    case, you should update the system software again.

 9. The settings of the camera will remain intact during and after the update.
    It is recommended, however, to reset certain parts of the configuration to
    the factory defaults, while keeping the other parts of the current
    configuration. If conflicts are detected while opening camera pages, warning
    messages will inform you about these conflicts.

    When resetting the configuration to factory defaults, the network, audio,
    and security settings should not be reset to factory defaults as this may
    render the camera unreachable.



* Files-Overview

    Bytes md5sum                            Name
--------------------------------------------------------------------------
 10804031 3ecb88e113c53a753d921a19d4adcc2b  MX_system_cn_3_5510.mpl
 11582271 c6b3bc88650341ca9240047787dad7a3  MX_system_de_3_5510.mpl
 11594559 fe34124d072795cd13d17cd74c10910b  MX_system_es_3_5510.mpl
 11340607 bcffcf17fcec1fb218be654b4cc92356  MX_system_fr_3_5510.mpl
 11701055 f7d087695c44bed78b933eceb9cd4b62  MX_system_it_3_5510.mpl
 11012927 f77d35a53e3f4150e04cdcbb1285e622  MX_system_jp_3_5510.mpl
 10533695 bf1a9687be9692765c8da28e23e23cf2  MX_system_ru_3_5510.mpl
