                  =============================
                  MOBOTIX FIRMWARE UPDATE NOTES
                  =============================


* General Information

  Date:           2018-02-07
  Release:        MX-V5.0.2.14

  For Hardware: MOBOTIX Network Cameras c26, i26, p26, v26, D26, M26, Q26, D16,
  M16, M16-Thermal, S16 and V16 with Thermal Sensors and 6MP or 5MP Image
  Sensors

  Manufacturer:   MOBOTIX AG
                  Kaiserstrasse
                  67722 Langmeil
                  GERMANY
                  http://www.mobotix.com/


* General Notes

This is an improved customer version for the MOBOTIX cameras c26, i26, p26, v26,
D26, M26, Q26, D16, M16, M16-Thermal, S16 and V16 with Thermal Sensors and 6MP
or 5MP Image Sensors.

This update will NOT work on older cameras.

News about this software release can be found under this address:

   http://www.mobotix.com/


* Updating the Camera Software

 1. Download the file MX_system_5_0214.mpl to your computer.

 2. Make sure that the file has been transferred completely. Please find the MD5
    checksums in the "Checksums_*.md5" files.

 3. Make sure that the camera fulfills the requirements listed above. Check
    the information under "Admin Menu > Hardware and Release Information" on the
    camera.

 4. Make sure that you are connected directly to the camera, without any proxy
    server in-between. Disable any proxy servers. Microsoft Internet Explorer:
    "Tools > Internet Options > Connections (tab) > Settings (in LAN Settings) >
    Proxy Server".

 5. Restart the camera.

 6. Log onto the camera as administrator, open "Admin Menu > Upload system
    Software" and read the Important Notes. Select the file
    MX_system_5_0214.mpl and start the upload.

    CAUTION:
       - Never disrupt the procedure while the camera is uploading or
         rewriting its flash memory. If this has happened anyhow, the camera
         will automatically boot the backup system (the title bar in the browser
         interface is red). The backup system only allows updating the system
         software.

       - The upload procedure may take several minutes, and up to 30 minutes
         when using an ISDN connection.

       - The camera LEDs will show a specific pattern while uploading.
         Please read the manual for the meaning.

       - During the procedure, the browser windows may not be updated
         properly.

 7. Upon completion of the upload, the camera will display a message. Read
    this message carefully.

 8. If the upload has finished successfully, restart the camera. If the upload
    was not successful, do not reboot the camera. Restart the upload process and
    wait until the upload has finished successfully.

    If the camera detects a faulty operating system, it will boot its backup
    operating system (the title bar in the browser interface is red); in this
    case, you should update the system software again.

 9. The settings of the camera will remain intact during and after the update.
    It is recommended, however, to reset certain parts of the configuration to
    the factory defaults, while keeping the other parts of the current
    configuration. If conflicts are detected while opening camera pages, warning
    messages will inform you about these conflicts.

    When resetting the configuration to factory defaults, the network, audio,
    and security settings should not be reset to factory defaults as this may
    render the camera unreachable.
