## Entering MxThinClient Settings

Name
The name for the MxThinClient that is shown in the Device bar. You can freely select the name and it does not have to be unique.

Serial Number
The serial number is the factory-defined IP address that is printed on the housing of the MxThinClient. Remember that you need to enter the number correctly because it represents the address at which the MxThinClient is accessed in the MxMessageSystem.

URL (optional setting)
The IP address or DNS domain name at which the MxThinClient can be accessed.

User Name and Password (optional setting)
The access data on the MxThinClient that you entered when installing the MxThinClient.

Display Resolution
Here you can select the resolution that the camera’s live image uses when data is sent to the display unit. If the display unit does not support the desired format, the MxThinClient displays the message Resolution not supported on the monitor.

Camera Display Time
You can select how long the armed camera’s live image is displayed before the MxThinClient continues with displaying the normal sequence of configured image sources.
If you select Unlimited for the display length, the camera’s live image is displayed until the MxThinClient receives a new command, such as when an event is triggered when it receives MxMessages from other cameras/devices in the network.
If you want to stop the display of the camera’s live image before the set display length elapses, click on the icon. It appears when you move the mouse pointer over the name of the MxThinClient in the Device bar.