# The Components View

In the MOBOTIX Component View, you can manage File Servers that are used to store video recordings. You can also manage Smart Data Sources (license required) from which you can read transaction data, e.g. from POS systems or license plate recognition systems.

## File Server Settings

Stored images can be accessed in two ways: Access via the camera or directly to a file server where the recordings are stored. If access is to be direct, you can create recording paths here that can be assigned to the cameras. (See Entering and Editing Camera Data).

Name
Geben Sie hier einen Namen für den Dateiserver an. Unter diesem Namen kann der Pfad im Dialog Kamerakonfiguration als Aufzeichnungspfad ausgewählt werden.

Type

- Local
  Contains a local folder on this computer or on a connected network drive. You can either enter the folder path manually, drag&drop a folder to the text box or select the folder.
  Pfad: you must select the path that contains the recording folders created by the camera.
- Network Share
  The program directly accesses a shared folder on a file server. In this case, you need to enter the computer, the folder and the access data.
  File Server (IP): IP address or DNS name of the file server with the share.
  Directory: Name of the share on the file server.
  Important: Make sure that the path ends before the folder containing the factory IP address of the camera.
  User Name/Password: Access data for the network share.
- MOBOTIX NAS
  Data is accessed directly on a shared folder on a MOBOTIX NAS.
  File Server (IP): IP address or DNS name and port of the MOBOTIX NAS.
  Directory: Name of the share on the MOBOTIX NAS.
  Important: Make sure that the path ends before the folder containing the factory IP address of the camera.
  User Name/Password: Access data for the MOBOTIX NAS.

- MOBOTIX NAS (ONVIF)
  The ONVIF recordings are accessed on a MOBOTIX NAS.
  File Server (IP): IP address or DNS name of the file server.
  User Name/Password: Access data for the file server.

Enlarge Image

## Smart Data Settings

Edit here Smart Data sources (e.g. POS systems or license plate recognition systems).

Description
Enter a meaningful name for the Smart Data Source here. Under this name, the source can be identified and selected in the MxMC for research.

Name
Enter the name (without spaces) for the Smart Data Source exactly as it was assigned in its configuration (also without spaces).

Smart Data Type
Select the type of Smart Data device here.

Data Source
Select the camera in which the Smart Data source (identified by the name given above) stores its transaction data.

Video Source
Select the camera that provides recordings for the transaction data. The video source and the data source do not have to be identical.

Enlarge Image

## MxThinClient-Settings

Edit the MxThinClient setting here. The MxThinClient is a compact solution for displaying the live image of a MOBOTIX camera on a monitor or TV set with HDMI connection.

Name
Enter the name for the MxThinClient here.

URL
Enter the URL or IP address of the ThinClient.

User Name
Enter the user name of the MxThinClient user here.

Password
Enter the password of the ThinClient user here.

Display resolution
Select the resolution of the camera image to be displayed on the monitor of the MxThinClient.

Camera display
Select here how long the assigned camera image should be displayed on the monitor of the ThinClient. After the selceted time period tht ThinClient will display the configured setting (e. g. sequences, still images etc.).

Bild vergrößern

###### Copyright © 2019 MOBOTIX AG. All rights reserved.