## Bandwidth

Using MxManagementCenter, you can access cameras from different locations. To do so, you need to define different environments, which will store the access data for the individual cameras. By assigning a bandwidth to an environment, you can specify how the images are pulled from the cameras given different connection speeds. This basically controls how the images can be displayed for live viewing and event research. Note that you can temporarily overwrite the bandwidth setting without actually changing the setting for the current environment.

- HiRes: The images are transferred using the current camera settings.
- LoRes: The images provided are in CIF size and with low frame rate.
- Unchanged: If you have changed the bandwidth several times, you can use this setting to quickly revert to the camera settings for this environment.