# Camera Feature Overview

MxMC allows MOBOTIX MOVE cameras and third-party cameras providing an ONVIF S-compatible interface to be integrated and operated. However, the full range of MxMC features is not available for all camera types.
The following table briefly lists the functions that be used with the different camera types.

Function | MOBOTIX Camera | MOBOTIX MOVE | ONVIF Camera
--- | --- | --- | ---
Camera Configuration | yes | no | no
Alarm Processing | yes | no | no
Recording Access | unlimited | only via MOBOTIX NAS | only via MOBOTIX NAS
Recording Playback | unlimited | only forward playback | only forward playback
Export | unlimited | only as MJPEG and H.264 (H.264 with corresponding license) | only as MJPEG and H.264 (H.264 with corresponding license)
Research View | yes | only for marked events | only for marked events
Special Search Functions (post-VM, histogram, Smart Data) | yes | no | no
Check System Security | yes | no | no
PTZ | Camera PTZ | mechanical PTZ | mechanical PTZ
Subsequent Equalization of Hemispherical Images | yes | no | no
Live Recorder | yes | no | no
Camera Groups | unlimited | group functions | group functions
Door Station Functions and Switching Functions | yes | no | no
MxThinClient Devices | yes | no | no
Snapshots | yes | no | no

###### Copyright © 2019 MOBOTIX AG. All rights reserved.