## Export Bar

The Export bar provides a quick and easy way to take camera recordings and MXG clips by dragging and dropping and create a list of recordings for subsequent exporting. From the bar, you can export recording time ranges as combined clips. You can add the clips in the Playback view, in Grid Playback, in the Research view and in the Smart Data View. The Export bar is not automatically deleted after an export. It is deleted when the program is closed.

### Adding Clips for Exporting

#### Adding Clips for Exporting in the Playback View

1. Drag the desired camera or the desired clip from the camera bar or from the Device bar.
2. Find the recording you are interested in.
3. Mark the start of the time range by clicking on the gray flag on the left . Play the recording until you have reached the end of the clip you want to export. Mark the end of the time range by clicking on the gray flag on the right . Both flags are now green.
   You can set the end marker first (gray flag on the right), then play the recording from the beginning so you can set the start marker (gray flag on the left) at the desired point.
4. Click on the image of the recording and maintain the position until you see a scaled-down image.
5. Drag this image to the Alarm bar (regardless of whether or not it is open). The Alarm bar automatically turns into the Export bar, allowing you to place the image there.
   Another option is to: Activate the Alarm bar. Click on the lower frame border of the open Alarm bar. The Export bar opens. Click on . The selected time range will be copied to the Export bar.

#### Adding Clips for Exporting in Grid Playback

The Export bar in Grid Playback is the best way to combine sequential time ranges of different cameras. For example, you can use it to follow one person who passes by several cameras.

1. Drag the desired camera to the focus window in the grid and find the relevant recording.
2. Mark the start of the time range by clicking on the gray flag on the left . Play the recording until you have reached the end of the clip you want to export. Mark the end of the time range by clicking on the gray flag on the right . Both flags are now green.
3. Click on the image of the recording in the focus window and maintain the position until you see a scaled-down image. Drag this image to the Alarm bar (regardless of whether or not it is open). The Alarm bar automatically turns into the Export bar, allowing you to place the image there.
4. After you have set the end marker of the time range, the recordings of all other cameras will reposition to show the same time. Drag the camera with the next recording in the sequence of events into the focus window. Mark the start and the end of the clip as described above, then drag the recording into the Export bar.
5. Repeat these steps until you have added all recordings you want to export.

Note that you can also add time ranges from several cameras in the Export bar.

1. Simply drag the desired camera group from the Group bar or from the Device bar and search for the relevant recording.
2. Mark the start and the end of the clip as described above. The recordings of the other cameras will reposition accordingly.
3. Right-click on Export . A selection box with a checkmark appears in the top left corner of the recordings. If you do not want to add the recording range of a specific camera to the list, deactivate that camera.
4. Click on the image of the recording in the focus window and maintain the position until you see a scaled-down image. Drag this image to the Alarm bar (regardless of whether or not it is open). The Alarm bar automatically turns into the Export bar, allowing you to place the image there. This means that all selected clips have been added to the Export bar.
5. Repeat these steps until you have added all time ranges you want to export.

#### Adding Clips for Exporting in the Research View

In the Research view, you can add recorded event sequences to the list. The length of the event sequences is currently 10 seconds.

1. Set filters by camera, by group or by event type as needed.
2. Right-click on Export . A selection box appears on the event images in the top left corner. Select the desired events by clicking on the corresponding selection boxes.
3. Open the Export bar by clicking on the lower frame border of the open Alarm bar. Click on an event image and maintain the position until you see a scaled-down event image. Drag this image to the Export bar. The clips of all selected event images are added to the Export bar.
   Another option is to: In the Export bar, click on . The clips of all selected event images are added to the Export bar.
4. If needed, you can set new filters and add more event images to the Export bar.

#### Adding Clips for Exporting in the Smart Data-View

You can add clips for the individual Smart Data transactions to the Export bar. The default clip length is ten seconds on either side of the transaction timestamp, that is, for a total of 20 seconds.

1. Right-click on Export . A selection box appears on the preview images in the top left corner. Select the desired transactions by clicking on the corresponding selection boxes.
2. Open the Export bar by clicking on the lower frame border of the open Alarm bar. Click on an preview image and maintain the position until you see a scaled-down preview image. Drag this image to the Export bar. The clips of all selected preview images are added to the Export bar.
   Another option is to: In the Export bar, click on . The clips of all selected preview images are added to the Export bar.

You can also add clips for the individual preview images of the selected transaction to the Export bar. To do so, drag the transaction preview image in the Preview Image section and drop it on the Export bar.

### Editing Clips

If you have added a recording to the Export bar, for which you had activated distortion correction or zoom features during playback, you can choose to export the clip with or without PTZ settings. Likewise, you can export the clip with or without audio. To do so, move the mouse pointer over the recording in the Export bar. Three icons appear:

- : Clip is exported with PTZ.
  Click on to export the clip without PTZ. The icon is disabled.
- : By default, the clips are exported with audio (provided that audio had been recorded).
  To export without audio, click on . The icon is disabled.
- : Note that you can review the clips before exporting by playing back individual clips directly in the Export bar. Click on to do so.

Right-click on a clip to open a context menu with these functions: Manually adjust time range, activate/deactivate audio and PTZ for all clips, duplicate a clip, delete one or all clips.

### Exporting

Click on Export , then select MOBOTIX to export an MXG clip. Select a different profile to create an AVI file. Select a target folder in the Export dialog and enter a file name. Activate the Automatically import after export checkbox to automatically add the MXG clips to the Export bar after exporting.