# Door Station Wizard

The Door Station wizard will guide you through the basic configuration of a selected door station.

Also see:

- Door Station Settings
- Operate Door Stations

Basic requirements

- Make sure that the devices run the latest software otherwise the configuration could fail.
- Additional door stations (including S1x, S2x cameras) to be configured must be listed in the Device Bar.
- Apply the default password "meinsm" to all door stations. To do so, you can use the Secure System Wizard.
- Apply the default password "meinsm" to MxDisplay devices to be configured.

Step by step

1. To open the Wizards & Tools view, right-click on the navigation key in the Command bar. Select the Wizards & Extras view.
2. Select the related door station (camera) Device bar or the Camera/Group bar and click Initialize Door Station. The Door Station Wizard starts up.
3. Read the introduction text and make sure you meet the basic requirements for the further configuration. Click Continue.
4. Select the devices you want to configure and click Continue. The Selected devices will be configured. This can take while.
   Note:
   Only devices with suitable software can be selected. The Master door station cannot be deselected.

5. Check the summary of the configured devices and click Continue.
6. Follow the next remaining configuration steps and click Finish.
   - Initialization of door station RFID module
   - Add MxBell as remote Station
   - Define all relationships between addresses and remote stations
   - Configure I/O-wiring
   - Final configuration of all door station (cameras)
   - Setup MxDisplay