# Alarm Bar And Export Bar

The bar at the bottom of the MxManagementCenter contains the Alarm and Export bar. The Alarm bar turns red when there is an unacknowledged alarm event. This happens only if the Alarms option has been activated in the Camera Configuration dialog box and if the event types responsible for triggering an alarm have been activated.
Clicking on the bottom frame border of the open Alarm bar will take you from the Alarm bar to the Export bar. Using drag & drop, the Export bar provides a quick and easy way to collect recordings for subsequent exporting.

### Alarm Bar

### Recognizing and Acknowledging New Alarms

If the bar is hidden, new alerts will be indicated by a red frame border . If the bar is open, the Info bar of the event image turns red. A ringing at the door bell will color the bar in green .
To acknowledge a new alarm, right-click on the event image and select Confirm. To acknowledge all new alarms at once, select Confirm All.

### Filtering the Display of Alarm Images

The alarm images in the Alarm bar are sorted chronologically. You can filter the event images by camera, by group or by event type. There are two sliders for this purpose: the group/camera slider and the event type slider. To set the filter, move the sliders until you see the desired results:

- Group/Camera: Group , camera
- Event Type: All , MxActivitySensor , Video Motion Sensor , Behavioral Detection , Shock Detector , Illumination , Microphone , PIR Sensor , Temperature , Internal Events , MxMessageSystem , Meta Events , Signal Input Events , Time Events , Bell Events , Voice Mailbox Messages , Door Station Events , RFID Rejected , PIN Rejected .

### Playing Back Recordings

- You can play back the recording associated with an alarm directly from the Alarm bar (instant playback). To do so, move the mouse pointer over the alarm image. Three icons appear. Click on .
- To play back the alarm in the Playback view, move the mouse pointer over the alarm image. Click on to switch to the Playback view.

### Deactivating Alarms

You can use the Camera Configuration dialog box or the Alarm bar to deactivate alarms.

- Deactivating alarms for a specific camera and event type:
  Right-click on the desired alarm image and select Deactivate As Alarm.
- Disable alarms for all event types of a camera:
  Right-click on an alarm image and select Deactivate All Alarms of This Camera.

### Export Bar

The Export bar can be opened in all views, and clips that have already been added can be edited in the bar. To do so, right-click on a clip. A shortcut menu with the following functions opens:

- : Manually adjusting the time range
- : Turning audio and PTZ on or off for all clips
- : Duplicating a clip
- : Deleting one or all clips

You can add the clips to be exported in the Playback view, in Grid Playback and in the Research view. Note that the Export bar will not be deleted automatically after exporting, but only when closing the application.

###### Copyright © 2019 MOBOTIX AG. All rights reserved.